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Please use this tool to upgrade the firmware
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Open this tool, can get this:
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 click the red part. 
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And then click “Start burn”
 During burning, do not plug out the camera. Otherwise will damage the camera. 
